|  |  |
| --- | --- |
| **Lighting – Technical Specification Sheet for XXX Theatre** | |
| **Lighting Control Board**   * Strand Tempus M 24 with FX unit   **Dimmers**   * L.S.C. Tour Series – 24 channels x 2.4 Kilowatt each channel * L.S.C. Tour Series – 12 channels x 2.4 Kilowatt each channel   **Power Supply**   * 200 Amps 3 Phase   **Lanterns**  Fresnels   * 18x Selecon SF 1000 - 1kw * 36 x Strand Pattern 123 - 500watt * 8x Strand Pattern 45 - 500kw * 8x Strand Pattern 743 - 1kw * 4 x Strand Pattern 243 - 2kw   Profiles   * 10 x C.C.T. Axial 30' zoom-1kw * 6 x Strand Pattern 264 -1kw * 4 x Strand Pattern 263 - 1kw * 20 x Strand 23 - 500watt * 4 x Strand 23 square gobo- 500watt * 18 x Strand 23N - 500watt   Flood Lights   * 6 x SB/63x8(Ground row Cyclorama) - 150watt * 2 x SB/63x4(Ground row Cyclorama) - 500watt * 28x Strand Pattern 60 - 500watt   Follow spots   * 2 x Strand Pattern 293 - 2kw * 2 x Strand Pattern 93 - 2kw   PAR cans   * 12 x PAR 64 narrow - 1kw * 6 x PAR 64 medium – 1 kw | **Cables**   * 2 x 1 metre extension leads * 11 x 2 metre extension leads * 4 x 3 metre extension leads * 2 x 4.5 metre extension leads * 12 x 5 metre extension leads * 1 x 8 metre extension leads * 4 x 9 metre extension leads * 2 x 10 metre extension leads   **Accessories**   * 1 x Floor Stand * 6 x power boards (4 outlets)   **Patching System**  US Well  12 outlets  Numbers: 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56  DS Well  12 outlets  Numbers: 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36  Floor Traps – DS Edge  6 outlets  Numbers: 15, 16, 17, 18, 19, 20 |
| *Sample of simple Technical Specifications Sheet for Lighting at a live venue* | |