|  |
| --- |
| **Lighting – Technical Specification Sheet for XXX Theatre** |
| **Lighting Control Board** * Strand Tempus M 24 with FX unit

**Dimmers** * L.S.C. Tour Series – 24 channels x 2.4 Kilowatt each channel
* L.S.C. Tour Series – 12 channels x 2.4 Kilowatt each channel

**Power Supply** * 200 Amps 3 Phase

**Lanterns** Fresnels * 18x Selecon SF 1000 - 1kw
* 36 x Strand Pattern 123 - 500watt
* 8x Strand Pattern 45 - 500kw
* 8x Strand Pattern 743 - 1kw
* 4 x Strand Pattern 243 - 2kw

Profiles * 10 x C.C.T. Axial 30' zoom-1kw
* 6 x Strand Pattern 264 -1kw
* 4 x Strand Pattern 263 - 1kw
* 20 x Strand 23 - 500watt
* 4 x Strand 23 square gobo- 500watt
* 18 x Strand 23N - 500watt

Flood Lights * 6 x SB/63x8(Ground row Cyclorama) - 150watt
* 2 x SB/63x4(Ground row Cyclorama) - 500watt
* 28x Strand Pattern 60 - 500watt

Follow spots * 2 x Strand Pattern 293 - 2kw
* 2 x Strand Pattern 93 - 2kw

PAR cans* 12 x PAR 64 narrow - 1kw
* 6 x PAR 64 medium – 1 kw
 | **Cables*** 2 x 1 metre extension leads
* 11 x 2 metre extension leads
* 4 x 3 metre extension leads
* 2 x 4.5 metre extension leads
* 12 x 5 metre extension leads
* 1 x 8 metre extension leads
* 4 x 9 metre extension leads
* 2 x 10 metre extension leads

**Accessories*** 1 x Floor Stand
* 6 x power boards (4 outlets)

**Patching System**US Well 12 outletsNumbers: 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56 DS Well 12 outletsNumbers: 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36Floor Traps – DS Edge6 outletsNumbers: 15, 16, 17, 18, 19, 20 |
| *Sample of simple Technical Specifications Sheet for Lighting at a live venue* |